**QUESTIONS TO HAND IN – INTRODUCTION**

**NAME\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**LAB DAY/TIME\_\_\_\_\_\_\_\_\_\_ \_ \_\_**

**1.** A clerk in a hardware store can measure length with a ruler to the nearest ±1 mm. If he measures out a length of chain to be 50 cm, what is the percentage uncertainty in the measurement?

**2.** The same clerk measures out a 50 cm x 150 cm piece of screen. What is the best value for the area of the screen?

**3.** Assuming the uncertainty in each length is still ±1 mm, what is the percentage uncertainty in the area measurement?

**4.** A carpenter measures the placement of studs in a wall every 16 inches. When she tries to fit an 8 ft length of wallboard, how many studs should it cover, not counting the very first one?

**5.** Assuming that she can allow herself a total error of ± inch (half the width of a 2 x 4), what is the maximum uncertainty she can tolerate in the placement of each stud?